PLATE LABELS - KG TOUR (Karol G) BAND RISERS - Rev C patch (LOCKED 7/10)

HOW TO PRINT (Brother P-touch Editor):
1. EASIEST - native files: open lbx/<label>.lbx directly in P-touch Editor and hit print.
   Pre-set for 24mm tape (TZe-251 black/white), auto length, PT-D610BT.
2. Or: new label, 24mm tape, Insert > Image > pick the PNG, scale to tape height, print.
3. Or: use labels.csv with a database-merge layout (fields: label_line1 / label_line2).

WHICH LABEL GOES WHERE:
- input-feeds/*.png -> the plate where the home run from the rack/controller lands.
  Filename = zone__device-output__DMX-start. Matches the DMX & Rack Output Maps
  on stl.kg3.io/maps (blue pill = same rack/output, yellow pill = same DMX).
  R1 = Rack 1 (CSR) . R2 = Rack 2 (CSL) . PA = Pelican A (SR) . PB = Pelican B (SL)
- daisy-chain-LEFT / RIGHT -> every in/out plate inside a zone, arrow pointing the
  direction the chain flows (toward the next segment).

34 feed labels total: 22 Center (CS) + 6 SL + 6 SR.
Questions -> Kenny 615-904-5640
